;RSen_C_model##OTHER##;RSen_C_type##OTHER##;RSen_C_type_comments##OTHER##;RSen_C_description##OTHER##;RSen_C_code_article##OTHER##;RSen_C_length##LENGTH##MILLIMETERS;RSen_C_height##LENGTH##MILLIMETERS;RSen_C_depth##LENGTH##MILLIMETERS;ZZZ_V Component_01_description_Text##OTHER##;ZZZ_V Component_01_length_Length##LENGTH##MILLIMETERS;ZZZ_V Component_01_height_Length##LENGTH##MILLIMETERS;ZZZ_V Component_01_width_Length##LENGTH##MILLIMETERS;ZZZ_V Component_01_plane_Integer##OTHER##;ZZZ_V Component_01_X_Length##LENGTH##MILLIMETERS;ZZZ_V Component_01_Y_Length##LENGTH##MILLIMETERS;ZZZ_V Component_01_Z_Length##LENGTH##MILLIMETERS;ZZZ_Cut out_length_Length##LENGTH##MILLIMETERS;ZZZ_Cut out_width_Length##LENGTH##MILLIMETERS;ZZZ_Cut out_height_Length##LENGTH##MILLIMETERS;ZZZ_Cut out_position_X_Length##LENGTH##MILLIMETERS;ZZZ_Cut out_position_Y_Length##LENGTH##MILLIMETERS;ZZZ_Parallel wall mounted_YesNo##OTHER##;ZZZ_Pendant - vertical mounted_YesNo##OTHER##;ZZZ_Recess depth_Length##LENGTH##MILLIMETERS;ZZZ_Recessed_YesNo##OTHER##;ZZZ_Surface mounted_YesNo##OTHER##;TBQen_C_offset_from_base_level##LENGTH##MILLIMETERS;TBQ_I Offset from base level_min##LENGTH##MILLIMETERS;TBQ_I Offset from base level_max##LENGTH##MILLIMETERS;ZZZ_Logo_plane_Integer##OTHER##;ZZZ_V Logo_FamilyType_Generic Models##OTHER##;ZZZ_Logo_Rotation about axis_Angle##ANGLE##DEGREES;ZZZ_Logo_X_Length##LENGTH##MILLIMETERS;ZZZ_Logo_Y_Length##LENGTH##MILLIMETERS;ZZZ_Logo_Z_Length##LENGTH##MILLIMETERS;ZZZ_V Clearance zone_back_Length##LENGTH##MILLIMETERS;ZZZ_V Clearance zone_bottom_Length##LENGTH##MILLIMETERS;ZZZ_V Clearance zone_front_Length##LENGTH##MILLIMETERS;ZZZ_V Clearance zone_left_Length##LENGTH##MILLIMETERS;ZZZ_V Clearance zone_right_Length##LENGTH##MILLIMETERS;ZZZ_V Clearance zone_top_Length##LENGTH##MILLIMETERS;RSen_C_material##OTHER##;ZZZ_V Component_01_material_Material##OTHER##;TBQ_I Default Emission_Heating##HVAC_POWER##WATTS;TBQ_I N-Value##OTHER##
mipr0.00911038 - trench radiator - 2 pipe_jaga_mini canal pro_lxhxd 1100x90x380 mm;Mini Canal Pro;2 pipe;Trench Radiator;MINI CANAL PRO H009 L110 B38;MIPR0.00911038;1100;90;380;convector;1100;90;380;2;0;0;0;1100;380;90;0;0;0;0;90;1;1;0;0;0;1;RSen_55_GM_FB_logo - SH_jaga : standard;0;0;0;0;0;0;0;0;0;0;RSen_x_rgb 241 236 225 T00 white 101_gen;RSen_x_rgb 241 236 225 T00 white 101_gen;459;0
